# oscam.dvbapi

Section: File Formats (5)
Index Return to Main Contents

## NAME

oscam.dvbapi - DVB API configuration file for OSCam

## SYNOPSIS

DVBAPI settings, first match - first used

## DESCRIPTIONS

P: [CAID]:[provider ID]:[service ID]:[ECM PID]:[CHID] [force]:[PIDx] priority

  set priority, continue = 1: proceed with priority, recommended for
  pay-per-view services / EMMs (use carefully), although local SCs
  will be prioritised higher, default:none

I: [CAID]:[provider ID]:[service ID]:[ECM PID]:[CHID] [PIDx] ignore

  set ignore

J: [CAID]:[provider ID]:[service ID]:[ECM PID] joined CAID:joined provider ID:joined ECM PID

  join to another ECM PID

A: ::service ID:[PMT PID] :[provider ID][:][ECM PID]

  set a dummy ECM request with CAID FFFF for services with a constant CW shown as unencrypted service (for STBs with PMT PID support only)

A: ::service ID:[video PID] :[provider ID][:][ECM PID]

  set a dummy ECM request with CAID FFFF for services with a constant CW shown as unencrypted service (for STBs without PMT PID support only)

X: [CAID]:[provider ID]:[service ID]:[ECM PID]

  add decoding on an extra demux index on the same CA device (Multi ECM) (not support on all STBs)

D: [CAID]:[provider ID]:[service ID]:[ECM PID] delay

  set delay in milli-seconds writing CWs

M: [CAID]:[provider ID]:[service ID]:[ECM PID] target CAID[:][target provider ID]

  mapping

S: [device] [PMT file name]

  set DVB API device name and PMT file name (valid for STAPI only)

L: [CAID]:[provider ID]:[service ID]:[ECM PID] length

  set ECM length in hexadecimal

## ANNONTATIONS

Please use Unix text file format only.

## EXAMPLES

P: 0100:123456 # prioritise CAID 0100 with provider 123456

P: :1234 # prioritise ECM with provider ID 1234 on
# on any CAID and service

P: 0200 # prioritise CAID 0200

P: 0300::9ABC # prioritise CAID 0300 on service 9ABC only

P: 0400 1 # prioritise CAID 0400 for pay-per-view services
P: : 1 # prioritise for EMMs

M: 0500 0600:123456 # map CAID 0500 to provider ID 123456 with
# CAID 0600

D: 0700 200 # wait 200 ms before writing CW for CAID 0700

I: :654321 # ignore provider ID 654321 for every CAID and
# service

I: 0 # ignore every CAID that was not handled before

L: 0800 8e # ECM length for CAID 0800 to 8e (hexadecimal)

## SEE ALSO

list_smargo(1), oscam(1), oscam.ac(5), oscam.cacheex(5), oscam.cert(5), oscam.conf(5), oscam.fakecws(5), oscam.guess(5), oscam.ird(5), oscam.provid(5), oscam.ratelimit(5), oscam.server(5), oscam.services(5), oscam.srvid(5), oscam.srvid2(5), oscam.user(5), oscam.whitelist(5)

## Index

NAME
SYNOPSIS
DESCRIPTIONS
ANNONTATIONS
EXAMPLES
SEE ALSO