oscam.dvbapi(5) 				       File Formats Manual					  oscam.dvbapi(5)



NAME
       oscam.dvbapi - DVB API configuration file for OSCam

SYNOPSIS
       DVBAPI settings, first match - first used

DESCRIPTIONS
       P: [CAID]:[provider ID]:[service ID]:[ECM PID]:[CHID] [force]:[PIDx] priority
	   set priority, continue = 1: proceed with priority, recommended for
	   pay-per-view services / EMMs (use carefully),  although local SCs
	   will be prioritised higher, default:none

       I: [CAID]:[provider ID]:[service ID]:[ECM PID]:[CHID] [PIDx] ignore
	   set ignore

       J: [CAID]:[provider ID]:[service ID]:[ECM PID] joined CAID:joined provider ID:joined ECM PID
	   join to another ECM PID

       A: ::service ID:[PMT PID] :[provider ID][:][ECM PID]
	   set a dummy ECM request with CAID FFFF for services with a constant CW shown as unencrypted service (for STBs with PMT
	  PID support only)

       A: ::service ID:[video PID] :[provider ID][:][ECM PID]
	   set a dummy ECM request with CAID FFFF for services with a constant CW shown as unencrypted service (for STBs  without
	  PMT PID support only)

       X: [CAID]:[provider ID]:[service ID]:[ECM PID]
	   add decoding on an extra demux index on the same CA device (Multi ECM) (not support on all STBs)

       D: [CAID]:[provider ID]:[service ID]:[ECM PID] delay
	   set delay in milli-seconds writing CWs

       M: [CAID]:[provider ID]:[service ID]:[ECM PID] target CAID[:][target provider ID]
	   mapping

       S: [device] [PMT file name]
	   set DVB API device name and PMT file name (valid for STAPI only)

       L: [CAID]:[provider ID]:[service ID]:[ECM PID] length
	   set ECM length in hexadecimal

ANNONTATIONS
       Please use Unix text file format only.

EXAMPLES
	P: 0100:123456	     # prioritise CAID 0100 with provider 123456

	P: :1234	     # prioritise ECM with provider ID 1234 on
			     # on any CAID and service

	P: 0200 	     # prioritise CAID 0200

	P: 0300::9ABC	     # prioritise CAID 0300 on service 9ABC only

	P: 0400 1	     # prioritise CAID 0400 for pay-per-view services

	P: : 1		     # prioritise for EMMs

	M: 0500 0600:123456  # map CAID 0500 to provider ID 123456 with
			     # CAID 0600

	D: 0700 200	     # wait 200 ms before writing CW for CAID 0700

	I: :654321	     # ignore provider ID 654321 for every CAID and
			     # service

	I: 0		     # ignore every CAID that was not handled before

	L: 0800 8e	     # ECM length for CAID 0800 to 8e (hexadecimal)

SEE ALSO
       list_smargo(1),	oscam(1),  oscam.ac(5), oscam.cacheex(5), oscam.cert(5), oscam.conf(5), oscam.fakecws(5), oscam.guess(5),
       oscam.ird(5), oscam.provid(5), oscam.ratelimit(5), oscam.server(5),  oscam.services(5),	oscam.srvid(5),  oscam.srvid2(5),
       oscam.user(5), oscam.whitelist(5)



														  oscam.dvbapi(5)
