Detect:
MHz: desired clockspeed or auto if autospeedbox is checked(auto only applies to smargo or dreambox yet)
Autospeed:Sets mhz according to atr for smargo readers and dreambox internal readers. Default is checked
Card MHz: Dreambox Mipsel: 2700, PPC: 3150, DM7025: 8300 ELSE set wanted cardinit speed. Default 357
##TPLREADERCONFIGRSAKEY## ##TPLREADERCONFIGDESKEY## ##TPLREADERCONFIGBOXKEY## ##TPLREADERPINCODE## ##TPLREADERCONFIGNANO##
Reset after No. ECM:
Deprecated:
##TPLREADERCONFIGNAGRA## ##TPLREADERCONFIGIRDETO## ##TPLREADERCONFIGVIACCESS## ##TPLREADERCONFIGVIDEOGUARD## ##TPLREADERCONFIGSC8IN1## ##TPLREADERCONFIGSMARGO## ##TPLREADERCOOLSTREAMBIT##